ACRO_BAL_PITCH,1
ACRO_BAL_ROLL,1
ACRO_OPTIONS,0
ACRO_RP_EXPO,0.3
ACRO_RP_P,4.5
ACRO_THR_MID,0
ACRO_TRAINER,2
ACRO_Y_EXPO,0
ACRO_YAW_P,4.5
AHRS_COMP_BETA,0.1
AHRS_CUSTOM_PIT,0
AHRS_CUSTOM_ROLL,0
AHRS_CUSTOM_YAW,0
AHRS_EKF_TYPE,3
AHRS_GPS_GAIN,1
AHRS_GPS_MINSATS,6
AHRS_GPS_USE,1
AHRS_ORIENTATION,0
AHRS_RP_P,0.2
AHRS_TRIM_X,0.009995357
AHRS_TRIM_Y,-0.009607053
AHRS_TRIM_Z,0
AHRS_WIND_MAX,0
AHRS_YAW_P,0.2
ANGLE_MAX,3000
ARMING_ACCTHRESH,0.75
ARMING_CHECK,1
ARMING_MIS_ITEMS,0
ARMING_RUDDER,2
ATC_ACCEL_P_MAX,110000
ATC_ACCEL_R_MAX,110000
ATC_ACCEL_Y_MAX,27000
ATC_ANG_LIM_TC,1
ATC_ANG_PIT_P,4.5
ATC_ANG_RLL_P,4.5
ATC_ANG_YAW_P,4.5
ATC_ANGLE_BOOST,1
ATC_INPUT_TC,0.15
ATC_RAT_PIT_D,0.002
ATC_RAT_PIT_FF,0
ATC_RAT_PIT_FLTD,20
ATC_RAT_PIT_FLTE,0
ATC_RAT_PIT_FLTT,20
ATC_RAT_PIT_I,0.135
ATC_RAT_PIT_IMAX,0.5
ATC_RAT_PIT_P,0.055
ATC_RAT_PIT_SMAX,0
ATC_RAT_RLL_D,0.002
ATC_RAT_RLL_FF,0
ATC_RAT_RLL_FLTD,20
ATC_RAT_RLL_FLTE,0
ATC_RAT_RLL_FLTT,20
ATC_RAT_RLL_I,0.135
ATC_RAT_RLL_IMAX,0.5
ATC_RAT_RLL_P,0.055
ATC_RAT_RLL_SMAX,0
ATC_RAT_YAW_D,0
ATC_RAT_YAW_FF,0
ATC_RAT_YAW_FLTD,0
ATC_RAT_YAW_FLTE,2.5
ATC_RAT_YAW_FLTT,20
ATC_RAT_YAW_I,0.018
ATC_RAT_YAW_IMAX,0.5
ATC_RAT_YAW_P,0.18
ATC_RAT_YAW_SMAX,0
ATC_RATE_FF_ENAB,1
ATC_RATE_P_MAX,0
ATC_RATE_R_MAX,0
ATC_RATE_Y_MAX,0
ATC_SLEW_YAW,6000
ATC_THR_MIX_MAN,0.1
ATC_THR_MIX_MAX,0.5
ATC_THR_MIX_MIN,0.1
AUTO_OPTIONS,0
AUTOTUNE_AGGR,0.1
AUTOTUNE_AXES,7
AUTOTUNE_MIN_D,0.001
AVOID_ACCEL_MAX,3
AVOID_ALT_MIN,0
AVOID_ANGLE_MAX,1000
AVOID_BACKUP_DZ,0.1
AVOID_BACKUP_SPD,0.75
AVOID_BEHAVE,0
AVOID_DIST_MAX,5
AVOID_ENABLE,3
AVOID_MARGIN,2
BARO_ALT_OFFSET,0
BARO_EXT_BUS,-1
BARO_FLTR_RNG,0
BARO_GND_TEMP,0
BARO_PRIMARY,0
BARO_PROBE_EXT,0
BARO1_DEVID,721674
BARO1_GND_PRESS,101135.3
BARO2_DEVID,0
BARO2_GND_PRESS,0
BARO3_DEVID,0
BARO3_GND_PRESS,0
BATT_MONITOR,0
BATT2_MONITOR,0
BATT3_MONITOR,0
BATT4_MONITOR,0
BATT5_MONITOR,0
BATT6_MONITOR,0
BATT7_MONITOR,0
BATT8_MONITOR,0
BATT9_MONITOR,0
BRD_ALT_CONFIG,0
BRD_BOOT_DELAY,0
BRD_IMU_TARGTEMP,-1
BRD_IMUHEAT_I,0.3
BRD_IMUHEAT_IMAX,70
BRD_IMUHEAT_P,200
BRD_IO_ENABLE,1
BRD_OPTIONS,1
BRD_PWM_COUNT,4
BRD_RTC_TYPES,1
BRD_RTC_TZ_MIN,0
BRD_SAFETY_MASK,16368
BRD_SAFETYENABLE,0
BRD_SAFETYOPTION,3
BRD_SBUS_OUT,0
BRD_SD_SLOWDOWN,0
BRD_SER1_RTSCTS,2
BRD_SER2_RTSCTS,2
BRD_SERIAL_NUM,0
BRD_TYPE,2
BRD_VBUS_MIN,4.3
BRD_VSERVO_MIN,0
BTN_ENABLE,0
CAM_AUTO_ONLY,0
CAM_DURATION,10
CAM_FEEDBACK_PIN,-1
CAM_FEEDBACK_POL,1
CAM_MAX_ROLL,0
CAM_MIN_INTERVAL,0
CAM_RELAY_ON,1
CAM_SERVO_OFF,1100
CAM_SERVO_ON,1300
CAM_TRIGG_DIST,0
CAM_TRIGG_TYPE,0
CAM_TYPE,0
CAN_D1_PROTOCOL,1
CAN_D2_PROTOCOL,1
CAN_LOGLEVEL,0
CAN_P1_DRIVER,0
CAN_P2_DRIVER,0
CAN_SLCAN_CPORT,0
CAN_SLCAN_SDELAY,1
CAN_SLCAN_SERNUM,-1
CAN_SLCAN_TIMOUT,0
CHUTE_ENABLED,0
CIRCLE_OPTIONS,1
CIRCLE_RADIUS,1000
CIRCLE_RATE,20
COMPASS_AUTO_ROT,2
COMPASS_AUTODEC,1
COMPASS_CAL_FIT,16
COMPASS_CUS_PIT,0
COMPASS_CUS_ROLL,0
COMPASS_CUS_YAW,0
COMPASS_DEC,-0.1196895
COMPASS_DEV_ID,131594
COMPASS_DEV_ID2,0
COMPASS_DEV_ID3,0
COMPASS_DEV_ID4,0
COMPASS_DEV_ID5,0
COMPASS_DEV_ID6,0
COMPASS_DEV_ID7,0
COMPASS_DEV_ID8,0
COMPASS_DIA_X,1
COMPASS_DIA_Y,1
COMPASS_DIA_Z,1
COMPASS_DIA2_X,0
COMPASS_DIA2_Y,0
COMPASS_DIA2_Z,0
COMPASS_DIA3_X,0
COMPASS_DIA3_Y,0
COMPASS_DIA3_Z,0
COMPASS_ENABLE,1
COMPASS_EXTERN2,0
COMPASS_EXTERN3,0
COMPASS_EXTERNAL,0
COMPASS_FLTR_RNG,0
COMPASS_LEARN,0
COMPASS_MOT_X,0
COMPASS_MOT_Y,0
COMPASS_MOT_Z,0
COMPASS_MOT2_X,0
COMPASS_MOT2_Y,0
COMPASS_MOT2_Z,0
COMPASS_MOT3_X,0
COMPASS_MOT3_Y,0
COMPASS_MOT3_Z,0
COMPASS_MOTCT,0
COMPASS_ODI_X,0
COMPASS_ODI_Y,0
COMPASS_ODI_Z,0
COMPASS_ODI2_X,0
COMPASS_ODI2_Y,0
COMPASS_ODI2_Z,0
COMPASS_ODI3_X,0
COMPASS_ODI3_Y,0
COMPASS_ODI3_Z,0
COMPASS_OFFS_MAX,1800
COMPASS_OFS_X,173.4011
COMPASS_OFS_Y,-3.995494
COMPASS_OFS_Z,-76.03139
COMPASS_OFS2_X,0
COMPASS_OFS2_Y,0
COMPASS_OFS2_Z,0
COMPASS_OFS3_X,0
COMPASS_OFS3_Y,0
COMPASS_OFS3_Z,0
COMPASS_OPTIONS,0
COMPASS_ORIENT,0
COMPASS_ORIENT2,0
COMPASS_ORIENT3,0
COMPASS_PMOT_EN,0
COMPASS_PRIO1_ID,131594
COMPASS_PRIO2_ID,0
COMPASS_PRIO3_ID,0
COMPASS_SCALE,0
COMPASS_SCALE2,0
COMPASS_SCALE3,0
COMPASS_TYPEMASK,0
COMPASS_USE,1
COMPASS_USE2,1
COMPASS_USE3,1
DEV_OPTIONS,0
DISARM_DELAY,10
EK3_ABIAS_P_NSE,0.003
EK3_ACC_BIAS_LIM,1
EK3_ACC_P_NSE,0.35
EK3_AFFINITY,0
EK3_ALT_M_NSE,2
EK3_BCN_DELAY,50
EK3_BCN_I_GTE,500
EK3_BCN_M_NSE,1
EK3_BETA_MASK,0
EK3_CHECK_SCALE,100
EK3_DRAG_BCOEF_X,0
EK3_DRAG_BCOEF_Y,0
EK3_DRAG_M_NSE,0.5
EK3_DRAG_MCOEF,0
EK3_EAS_I_GATE,400
EK3_EAS_M_NSE,1.4
EK3_ENABLE,1
EK3_ERR_THRESH,0.2
EK3_FLOW_DELAY,10
EK3_FLOW_I_GATE,300
EK3_FLOW_M_NSE,0.25
EK3_FLOW_USE,1
EK3_GBIAS_P_NSE,0.001
EK3_GLITCH_RAD,25
EK3_GND_EFF_DZ,4
EK3_GPS_CHECK,31
EK3_GSF_RST_MAX,2
EK3_GSF_RUN_MASK,3
EK3_GSF_USE_MASK,3
EK3_GYRO_P_NSE,0.015
EK3_HGT_DELAY,60
EK3_HGT_I_GATE,500
EK3_HRT_FILT,2
EK3_IMU_MASK,3
EK3_MAG_CAL,3
EK3_MAG_EF_LIM,50
EK3_MAG_I_GATE,300
EK3_MAG_M_NSE,0.05
EK3_MAG_MASK,0
EK3_MAGB_P_NSE,0.0001
EK3_MAGE_P_NSE,0.001
EK3_MAX_FLOW,2.5
EK3_NOAID_M_NSE,10
EK3_OGN_HGT_MASK,0
EK3_OGNM_TEST_SF,2
EK3_POS_I_GATE,500
EK3_POSNE_M_NSE,0.5
EK3_RNG_I_GATE,500
EK3_RNG_M_NSE,0.5
EK3_RNG_USE_HGT,-1
EK3_RNG_USE_SPD,2
EK3_SRC_OPTIONS,1
EK3_SRC1_POSXY,3
EK3_SRC1_POSZ,1
EK3_SRC1_VELXY,3
EK3_SRC1_VELZ,3
EK3_SRC1_YAW,1
EK3_SRC2_POSXY,0
EK3_SRC2_POSZ,1
EK3_SRC2_VELXY,0
EK3_SRC2_VELZ,0
EK3_SRC2_YAW,0
EK3_SRC3_POSXY,0
EK3_SRC3_POSZ,1
EK3_SRC3_VELXY,0
EK3_SRC3_VELZ,0
EK3_SRC3_YAW,0
EK3_TAU_OUTPUT,25
EK3_TERR_GRAD,0.1
EK3_VEL_I_GATE,500
EK3_VELD_M_NSE,0.5
EK3_VELNE_M_NSE,0.3
EK3_VIS_VERR_MAX,0.9
EK3_VIS_VERR_MIN,0.1
EK3_WENC_VERR,0.1
EK3_WIND_P_NSE,0.2
EK3_WIND_PSCALE,1
EK3_YAW_I_GATE,300
EK3_YAW_M_NSE,0.5
ESC_CALIBRATION,0
FENCE_ACTION,1
FENCE_ALT_MAX,100
FENCE_ALT_MIN,-10
FENCE_ENABLE,0
FENCE_MARGIN,2
FENCE_RADIUS,300
FENCE_TOTAL,0
FENCE_TYPE,7
FLIGHT_OPTIONS,0
FLOW_TYPE,0
FLTMODE_CH,5
FLTMODE1,0
FLTMODE2,0
FLTMODE3,0
FLTMODE4,5
FLTMODE5,0
FLTMODE6,3
FORMAT_VERSION,120
FRAME_CLASS,1
FRAME_TYPE,1
FRSKY_DNLINK_ID,27
FRSKY_DNLINK1_ID,20
FRSKY_DNLINK2_ID,7
FRSKY_UPLINK_ID,13
FS_CRASH_CHECK,1
FS_EKF_ACTION,1
FS_EKF_THRESH,0.8
FS_GCS_ENABLE,0
FS_GCS_TIMEOUT,5
FS_OPTIONS,16
FS_THR_ENABLE,1
FS_THR_VALUE,975
FS_VIBE_ENABLE,1
GCS_PID_MASK,0
GND_EFFECT_COMP,1
GPS_AUTO_CONFIG,0
GPS_AUTO_SWITCH,1
GPS_BLEND_MASK,5
GPS_BLEND_TC,10
GPS_CAN_NODEID1,0
GPS_CAN_NODEID2,0
GPS_COM_PORT,1
GPS_COM_PORT2,1
GPS_DELAY_MS,0
GPS_DELAY_MS2,0
GPS_GNSS_MODE,0
GPS_GNSS_MODE2,0
GPS_HDOP_GOOD,140
GPS_INJECT_TO,127
GPS_MIN_DGPS,100
GPS_MIN_ELEV,-100
GPS_NAVFILTER,8
GPS_POS1_X,0
GPS_POS1_Y,0
GPS_POS1_Z,0
GPS_POS2_X,0
GPS_POS2_Y,0
GPS_POS2_Z,0
GPS_PRIMARY,0
GPS_RATE_MS,200
GPS_RATE_MS2,200
GPS_RAW_DATA,0
GPS_SAVE_CFG,2
GPS_SBAS_MODE,2
GPS_SBP_LOGMASK,-256
GPS_TYPE,2
GPS_TYPE2,0
GPS1_CAN_OVRIDE,0
GPS2_CAN_OVRIDE,0
GUID_OPTIONS,0
GUID_TIMEOUT,3
INITIAL_MODE,0
INS_ACC_BODYFIX,2
INS_ACC_ID,1246218
INS_ACC2_ID,1114634
INS_ACC2OFFS_X,0.3375648
INS_ACC2OFFS_Y,0.7981029
INS_ACC2OFFS_Z,0.7864324
INS_ACC2SCAL_X,1.006612
INS_ACC2SCAL_Y,1.034898
INS_ACC2SCAL_Z,1.044342
INS_ACCEL_FILTER,20
INS_ACCOFFS_X,0.1232594
INS_ACCOFFS_Y,0.008893246
INS_ACCOFFS_Z,-0.3708665
INS_ACCSCAL_X,1.001282
INS_ACCSCAL_Y,0.9919199
INS_ACCSCAL_Z,0.9941608
INS_ENABLE_MASK,127
INS_FAST_SAMPLE,1
INS_GYR_CAL,1
INS_GYR_ID,2163722
INS_GYR2_ID,2228490
INS_GYR2OFFS_X,0.009335626
INS_GYR2OFFS_Y,0.01090964
INS_GYR2OFFS_Z,-0.01376853
INS_GYRO_FILTER,20
INS_GYRO_RATE,0
INS_GYROFFS_X,0.007139436
INS_GYROFFS_Y,0.02452319
INS_GYROFFS_Z,0.005148736
INS_HNTCH_ENABLE,0
INS_LOG_BAT_CNT,1024
INS_LOG_BAT_LGCT,32
INS_LOG_BAT_LGIN,20
INS_LOG_BAT_MASK,0
INS_LOG_BAT_OPT,0
INS_NOTCH_ENABLE,0
INS_POS1_X,0
INS_POS1_Y,0
INS_POS1_Z,0
INS_POS2_X,0
INS_POS2_Y,0
INS_POS2_Z,0
INS_STILL_THRESH,2.5
INS_TRIM_OPTION,1
INS_USE,1
INS_USE2,1
LAND_ALT_LOW,1000
LAND_REPOSITION,1
LAND_SPEED,50
LAND_SPEED_HIGH,0
LGR_DEPLOY_ALT,0
LGR_DEPLOY_PIN,-1
LGR_DEPLOY_POL,0
LGR_OPTIONS,3
LGR_RETRACT_ALT,0
LGR_STARTUP,0
LGR_WOW_PIN,-1
LGR_WOW_POL,0
LOG_BACKEND_TYPE,1
LOG_BITMASK,176126
LOG_DISARMED,0
LOG_FILE_BUFSIZE,16
LOG_FILE_DSRMROT,0
LOG_FILE_MB_FREE,500
LOG_FILE_TIMEOUT,5
LOG_MAV_BUFSIZE,8
LOG_REPLAY,0
LOIT_ACC_MAX,500
LOIT_ANG_MAX,0
LOIT_BRK_ACCEL,250
LOIT_BRK_DELAY,1
LOIT_BRK_JERK,500
LOIT_SPEED,1250
MIS_OPTIONS,0
MIS_RESTART,0
MIS_TOTAL,5
MOT_BAT_CURR_MAX,0
MOT_BAT_CURR_TC,5
MOT_BAT_IDX,0
MOT_BAT_VOLT_MAX,0
MOT_BAT_VOLT_MIN,0
MOT_BOOST_SCALE,0
MOT_HOVER_LEARN,2
MOT_PWM_MAX,0
MOT_PWM_MIN,0
MOT_PWM_TYPE,0
MOT_SAFE_DISARM,0
MOT_SAFE_TIME,1
MOT_SLEW_DN_TIME,0
MOT_SLEW_UP_TIME,0
MOT_SPIN_ARM,0.1
MOT_SPIN_MAX,0.95
MOT_SPIN_MIN,0.15
MOT_SPOOL_TIME,0.5
MOT_THST_EXPO,0.65
MOT_THST_HOVER,0.125
MOT_YAW_HEADROOM,200
NTF_BUZZ_ON_LVL,1
NTF_BUZZ_PIN,0
NTF_BUZZ_TYPES,5
NTF_BUZZ_VOLUME,100
NTF_LED_BRIGHT,3
NTF_LED_LEN,1
NTF_LED_OVERRIDE,0
NTF_LED_TYPES,199
PHLD_BRAKE_ANGLE,3000
PHLD_BRAKE_RATE,8
PILOT_ACCEL_Z,250
PILOT_SPEED_DN,0
PILOT_SPEED_UP,250
PILOT_THR_BHV,0
PILOT_THR_FILT,0
PILOT_TKOFF_ALT,0
PLND_ENABLED,0
PSC_ACCZ_D,0
PSC_ACCZ_FF,0
PSC_ACCZ_FLTD,0
PSC_ACCZ_FLTE,20
PSC_ACCZ_FLTT,0
PSC_ACCZ_I,1
PSC_ACCZ_IMAX,800
PSC_ACCZ_P,0.5
PSC_ACCZ_SMAX,0
PSC_ANGLE_MAX,0
PSC_JERK_XY,5
PSC_JERK_Z,5
PSC_POSXY_P,1
PSC_POSZ_P,1
PSC_VELXY_D,0.5
PSC_VELXY_FF,0
PSC_VELXY_FLTD,5
PSC_VELXY_FLTE,5
PSC_VELXY_I,1
PSC_VELXY_IMAX,1000
PSC_VELXY_P,2
PSC_VELZ_D,0
PSC_VELZ_FF,0
PSC_VELZ_FLTD,5
PSC_VELZ_FLTE,5
PSC_VELZ_I,0
PSC_VELZ_IMAX,1000
PSC_VELZ_P,5
RALLY_INCL_HOME,1
RALLY_LIMIT_KM,0.3
RALLY_TOTAL,0
RC_OPTIONS,32
RC_OVERRIDE_TIME,3
RC_PROTOCOLS,1
RC_SPEED,490
RC1_DZ,20
RC1_MAX,1900
RC1_MIN,1100
RC1_OPTION,0
RC1_REVERSED,0
RC1_TRIM,1500
RC10_DZ,0
RC10_MAX,1900
RC10_MIN,1100
RC10_OPTION,0
RC10_REVERSED,0
RC10_TRIM,1500
RC11_DZ,0
RC11_MAX,1900
RC11_MIN,1100
RC11_OPTION,0
RC11_REVERSED,0
RC11_TRIM,1500
RC12_DZ,0
RC12_MAX,1900
RC12_MIN,1100
RC12_OPTION,0
RC12_REVERSED,0
RC12_TRIM,1500
RC13_DZ,0
RC13_MAX,1900
RC13_MIN,1100
RC13_OPTION,0
RC13_REVERSED,0
RC13_TRIM,1500
RC14_DZ,0
RC14_MAX,1900
RC14_MIN,1100
RC14_OPTION,0
RC14_REVERSED,0
RC14_TRIM,1500
RC15_DZ,0
RC15_MAX,1900
RC15_MIN,1100
RC15_OPTION,0
RC15_REVERSED,0
RC15_TRIM,1500
RC16_DZ,0
RC16_MAX,1900
RC16_MIN,1100
RC16_OPTION,0
RC16_REVERSED,0
RC16_TRIM,1500
RC2_DZ,20
RC2_MAX,1900
RC2_MIN,1100
RC2_OPTION,0
RC2_REVERSED,0
RC2_TRIM,1500
RC3_DZ,30
RC3_MAX,1900
RC3_MIN,1100
RC3_OPTION,0
RC3_REVERSED,0
RC3_TRIM,1500
RC4_DZ,20
RC4_MAX,1900
RC4_MIN,1100
RC4_OPTION,0
RC4_REVERSED,0
RC4_TRIM,1500
RC5_DZ,0
RC5_MAX,1900
RC5_MIN,1100
RC5_OPTION,0
RC5_REVERSED,0
RC5_TRIM,1500
RC6_DZ,0
RC6_MAX,1900
RC6_MIN,1100
RC6_OPTION,0
RC6_REVERSED,0
RC6_TRIM,1500
RC7_DZ,0
RC7_MAX,1900
RC7_MIN,1100
RC7_OPTION,0
RC7_REVERSED,0
RC7_TRIM,1500
RC8_DZ,0
RC8_MAX,1900
RC8_MIN,1100
RC8_OPTION,0
RC8_REVERSED,0
RC8_TRIM,1500
RC9_DZ,0
RC9_MAX,1900
RC9_MIN,1100
RC9_OPTION,0
RC9_REVERSED,0
RC9_TRIM,1500
RCMAP_PITCH,2
RCMAP_ROLL,1
RCMAP_THROTTLE,3
RCMAP_YAW,4
RELAY_DEFAULT,0
RELAY_PIN,54
RELAY_PIN2,55
RELAY_PIN3,-1
RELAY_PIN4,-1
RELAY_PIN5,-1
RELAY_PIN6,-1
RNGFND_FILT,0.5
RNGFND1_ADDR,0
RNGFND1_FUNCTION,0
RNGFND1_GNDCLEAR,5
RNGFND1_MAX_CM,700
RNGFND1_MIN_CM,20
RNGFND1_OFFSET,0
RNGFND1_ORIENT,25
RNGFND1_PIN,-1
RNGFND1_POS_X,0
RNGFND1_POS_Y,0
RNGFND1_POS_Z,0
RNGFND1_PWRRNG,0
RNGFND1_RMETRIC,1
RNGFND1_SCALING,3
RNGFND1_STOP_PIN,-1
RNGFND1_TYPE,20
RNGFND2_TYPE,0
RNGFND3_TYPE,0
RNGFND4_TYPE,0
RNGFND5_TYPE,0
RNGFND6_TYPE,0
RNGFND7_TYPE,0
RNGFND8_TYPE,0
RNGFND9_TYPE,0
RNGFNDA_TYPE,0
RSSI_TYPE,0
RTL_ALT,500
RTL_ALT_FINAL,0
RTL_ALT_TYPE,0
RTL_CLIMB_MIN,0
RTL_CONE_SLOPE,3
RTL_LOIT_TIME,5000
RTL_OPTIONS,0
RTL_SPEED,0
SCHED_DEBUG,0
SCHED_LOOP_RATE,400
SCHED_OPTIONS,0
SERIAL_PASS1,0
SERIAL_PASS2,-1
SERIAL_PASSTIMO,15
SERIAL0_BAUD,115
SERIAL0_PROTOCOL,2
SERIAL1_BAUD,57
SERIAL1_OPTIONS,0
SERIAL1_PROTOCOL,2
SERIAL2_BAUD,115
SERIAL2_OPTIONS,0
SERIAL2_PROTOCOL,5
SERIAL3_BAUD,115
SERIAL3_OPTIONS,0
SERIAL3_PROTOCOL,9
SERIAL4_BAUD,38
SERIAL4_OPTIONS,0
SERIAL4_PROTOCOL,5
SERIAL5_BAUD,57
SERIAL5_OPTIONS,0
SERIAL5_PROTOCOL,-1
SERVO_BLH_3DMASK,0
SERVO_BLH_AUTO,0
SERVO_BLH_DEBUG,0
SERVO_BLH_MASK,0
SERVO_BLH_OTYPE,0
SERVO_BLH_POLES,14
SERVO_BLH_PORT,0
SERVO_BLH_RVMASK,0
SERVO_BLH_TEST,0
SERVO_BLH_TMOUT,0
SERVO_BLH_TRATE,10
SERVO_DSHOT_ESC,0
SERVO_DSHOT_RATE,0
SERVO_RATE,50
SERVO_ROB_POSMAX,4095
SERVO_ROB_POSMIN,0
SERVO_SBUS_RATE,50
SERVO_VOLZ_MASK,0
SERVO1_FUNCTION,33
SERVO1_MAX,1900
SERVO1_MIN,1100
SERVO1_REVERSED,0
SERVO1_TRIM,1500
SERVO10_FUNCTION,0
SERVO10_MAX,1900
SERVO10_MIN,1100
SERVO10_REVERSED,0
SERVO10_TRIM,1500
SERVO11_FUNCTION,0
SERVO11_MAX,1900
SERVO11_MIN,1100
SERVO11_REVERSED,0
SERVO11_TRIM,1500
SERVO12_FUNCTION,0
SERVO12_MAX,1900
SERVO12_MIN,1100
SERVO12_REVERSED,0
SERVO12_TRIM,1500
SERVO13_FUNCTION,0
SERVO13_MAX,1900
SERVO13_MIN,1100
SERVO13_REVERSED,0
SERVO13_TRIM,1500
SERVO14_FUNCTION,0
SERVO14_MAX,1900
SERVO14_MIN,1100
SERVO14_REVERSED,0
SERVO14_TRIM,1500
SERVO15_FUNCTION,0
SERVO15_MAX,1900
SERVO15_MIN,1100
SERVO15_REVERSED,0
SERVO15_TRIM,1500
SERVO16_FUNCTION,0
SERVO16_MAX,1900
SERVO16_MIN,1100
SERVO16_REVERSED,0
SERVO16_TRIM,1500
SERVO2_FUNCTION,34
SERVO2_MAX,1900
SERVO2_MIN,1100
SERVO2_REVERSED,0
SERVO2_TRIM,1500
SERVO3_FUNCTION,35
SERVO3_MAX,1900
SERVO3_MIN,1100
SERVO3_REVERSED,0
SERVO3_TRIM,1500
SERVO4_FUNCTION,36
SERVO4_MAX,1900
SERVO4_MIN,1100
SERVO4_REVERSED,0
SERVO4_TRIM,1500
SERVO5_FUNCTION,0
SERVO5_MAX,1900
SERVO5_MIN,1100
SERVO5_REVERSED,0
SERVO5_TRIM,1500
SERVO6_FUNCTION,0
SERVO6_MAX,1900
SERVO6_MIN,1100
SERVO6_REVERSED,0
SERVO6_TRIM,1500
SERVO7_FUNCTION,0
SERVO7_MAX,1900
SERVO7_MIN,1100
SERVO7_REVERSED,0
SERVO7_TRIM,1500
SERVO8_FUNCTION,0
SERVO8_MAX,1900
SERVO8_MIN,1100
SERVO8_REVERSED,0
SERVO8_TRIM,1500
SERVO9_FUNCTION,0
SERVO9_MAX,1900
SERVO9_MIN,1100
SERVO9_REVERSED,0
SERVO9_TRIM,1500
SIMPLE,0
SR0_ADSB,0
SR0_EXT_STAT,0
SR0_EXTRA1,0
SR0_EXTRA2,0
SR0_EXTRA3,0
SR0_PARAMS,0
SR0_POSITION,0
SR0_RAW_CTRL,0
SR0_RAW_SENS,0
SR0_RC_CHAN,0
SR1_ADSB,0
SR1_EXT_STAT,1
SR1_EXTRA1,5
SR1_EXTRA2,5
SR1_EXTRA3,5
SR1_PARAMS,0
SR1_POSITION,1
SR1_RAW_CTRL,0
SR1_RAW_SENS,5
SR1_RC_CHAN,1
SR2_ADSB,0
SR2_EXT_STAT,0
SR2_EXTRA1,0
SR2_EXTRA2,0
SR2_EXTRA3,0
SR2_PARAMS,0
SR2_POSITION,0
SR2_RAW_CTRL,0
SR2_RAW_SENS,0
SR2_RC_CHAN,0
SR3_ADSB,0
SR3_EXT_STAT,0
SR3_EXTRA1,0
SR3_EXTRA2,0
SR3_EXTRA3,0
SR3_PARAMS,0
SR3_POSITION,0
SR3_RAW_CTRL,0
SR3_RAW_SENS,0
SR3_RC_CHAN,0
SR4_ADSB,0
SR4_EXT_STAT,0
SR4_EXTRA1,0
SR4_EXTRA2,0
SR4_EXTRA3,0
SR4_PARAMS,0
SR4_POSITION,0
SR4_RAW_CTRL,0
SR4_RAW_SENS,0
SR4_RC_CHAN,0
SRTL_ACCURACY,2
SRTL_OPTIONS,0
SRTL_POINTS,300
STAT_BOOTCNT,1
STAT_FLTTIME,0
STAT_RESET,0
STAT_RUNTIME,0
SUPER_SIMPLE,0
SYSID_ENFORCE,0
SYSID_MYGCS,255
SYSID_THISMAV,1
TCAL_ENABLED,0
TELEM_DELAY,0
TERRAIN_ENABLE,1
TERRAIN_OPTIONS,0
TERRAIN_SPACING,100
THR_DZ,100
THROW_MOT_START,0
THROW_NEXTMODE,18
THROW_TYPE,0
TUNE,0
TUNE_MAX,0
TUNE_MIN,0
VTX_ENABLE,0
WP_NAVALT_MIN,0
WP_YAW_BEHAVIOR,2
WPNAV_ACCEL,250
WPNAV_ACCEL_Z,100
WPNAV_JERK,1
WPNAV_RADIUS,30
WPNAV_RFND_USE,1
WPNAV_SPEED,500
WPNAV_SPEED_DN,150
WPNAV_SPEED_UP,250
WPNAV_TER_MARGIN,10
